# Specification:

|  |  |
| --- | --- |
| Layers | 2 |
| PCB Thickness | 1.6 |
| PCB Color | RED |
| Surface Finish | LeadFree HASL-RoHS |
| Copper Weight | 1oz |
| Flying Probe Test | Fully Test |
| Castellated Holes | NO |
| Clear whole board | Yes |
| Packaging | Sealed ESD Bag |
| Addon to the package | YES, LCSC Part # C721445 |

## Diagram Description automatically generatedA picture containing text, toy Description automatically generatedA picture containing shape Description automatically generatedShape Description automatically generated with low confidencePictures: